For 1990-2009 cars

Important:

• | Before servicing the following items, use the scribing procedure:

- | The strut mount

- | The strut bumper

- | The strut shield

- | The spring seat

- | The spring insulator

- | After completing the service, you will be able to return to the original camber setting. Then, inspect and adjust the toe.

• | Do not use the scribing procedure when servicing the following components:

- | Front Spring

- | Strut

- | Knuckle

- | Control Arm

- | Inspect or adjust the camber and the toe after completing the service.

1. Use a chisel in order to place a mark across the strut/knuckle interface (1).
2. Scribe the strut flange on the inboard side along the curve of the knuckle (2).
3. Using a sharp tool, scribe the knuckle along the lower outboard strut radius (3).
4. During reassembly, carefully match the marks to the components.