For 1990-2009 cars

### Removal Procedure

1. Remove the radio. Refer to Radio Replacement .
2. Disconnect the amplifier electrical connector (2).
3. Push upward on the amp (3) in order to disengage the amp from the bracket (1).
4. Slide the amp (3) out of the bracket (1).

### Installation Procedure

1. Slide the amp (3) into the bracket (1).
2. Ensure that the wiring harness is routed through the clip on the upper side of the bracket.
3. Connect the electrical connector (2).
4. Install the radio. Refer to Radio Replacement .