For 1990-2009 cars

• | If the ride is too soft, inspect for the following conditions:

- | Worn strut dampers

- | Incorrect or weak springs

• | Inspect for diagnostic trouble codes in the computer command ride system.

• | If the ride is too harsh, inspect for the following conditions:

- | Incorrect strut dampers

- | Incorrect springs

- | Excessive friction in control arm bushings

• | Inspect for diagnostic trouble codes in the computer command ride system.