For 1990-2009 cars

#### Tools Required

J 28585 Snap Ring Remover

1. Inspect the differential carrier internal gear assembly (693) for the following conditions:

• | Damaged or worn bushings

• | Plugged lube oil holes

• | Damaged case splines

• | Damaged or worn gear teeth

• | A damaged or worn park pawl assembly (694)

• | A damaged snap ring (692)

2. Install the differential carrier internal gear assembly (693) into the case. Align the park pawl assembly with the park pawl actuator assembly.
3. Use J 28585 or a long screwdriver in order to install the snap ring (692) into the case as shown.