For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 22610 Service Boot Clamp Installer

1. To remove the outer tie rod; refer to Rack and Pinion Outer Tie Rod End Replacement .
2. Remove the hex jam nut (2) from the inner tie rod assembly (1).
3. Remove the tie rod end clamp (2) from the rack and pinion boot (1).
4. Remove the boot clamp (1) from the rack and pinion boot (3) with side cutters.
5. Discard the boot clamp (1).

Important: Prior to removing the breather tube (2) or the rack and pinion boot (3), mark the location of the breather tube (2) on the gear assembly.

6. Remove the rack and pinion boot (3) and the breather tube (2).

### Assembly Procedure

#### Tools Required

J 22610 Service Boot Clamp Installer

1. Install the new boot clamp (1) onto the rack and pinion boot (3).
2. Prior to rack and pinion boot installation, apply grease to the inner tie rod assembly (2) and the rack and pinion gear assembly (1).
3. Install the rack and pinion boot (3) onto the inner tie rod assembly (2).
4. Align the breather tube with the mark made during removal and the molded nipple of the rack and pinion boot.
5. Install the rack and pinion boot (3) onto the gear assembly until the rack and pinion boot (3) is seated in the gear assembly groove.

Important: The rack and pinion boot (3) must not be twisted, puckered or out of shape in any way. If the rack and pinion boot (3) is not shaped properly, adjust the rack and pinion boot (3) by hand before installing the boot clamp.

6. Install the rack and pinion boot (3) onto the inner tie rod assembly (2).
7. Install the boot clamp (2) on the rack and pinion boot (1) with J 22610 .
8. Crimp the boot clamp (2).
9. Pinch the pliers together on the rack and pinion boot (1) in order to install the tie rod end clamp.
10. Install the hex jam nut (2) to the inner tie rod assembly (1).
11. To assemble the outer tie rod assembly; refer to Rack and Pinion Outer Tie Rod End Replacement .