For 1990-2009 cars

The Computer Command Ride system has the ability to display the following diagnostic codes:

Code | Description
--- | ---
Code 12 | Initialization
Code 23 | Left Front Actuator Position Error
Code 24 | Right Front Actuator Position Error
Code 25 | Left Rear Actuator Position Error
Code 26 | Right Rear Actuator Position Error
Code 31 | Lift/Dive Signal Error
Code 32 | Lateral Accelerator Switch Error
Code 33 | Driver Select Switch Input Error
Code 34 | Vehicle Speed Signal Error