For 1990-2009 cars

## Steering Shaft, Lower Bearing, and Jacket - Assemble - Off Vehicle Column Shift

#### Tools Required

J 23073-01 Shift Tube Installer

1. Apply synthetic grease to the exposed shaft engagement areas (1). Install the lower steering shaft assembly (2) to the race and upper shaft assembly.
2. Install the gear shift bowl shroud (7).
3. Install the gear shift bowl assembly (6).
4. Install the shift lever spring (5).
5. Install the wave washer (4).
6. Install the lock plate (3).
7. Install the thrust washer (2).
8. Install the shift tube retaining ring (1).
9. Install the shift tube assembly (1) using J 23073-01 .
10. Install the steering column housing support assembly (4) with the dimmer switch rod (3) still connected.
11. Install the 4 torx head screws (2).

Tighten
Tighten the screws to 2 N·m (18 lb in).

12. Install the shift lever gate (1) secure with 2 oval head cross recess screws (6).

Tighten
Tighten the screws to 1 N·m (9 lb in).

13. Install the steering shaft assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

14. Install the adapter and bearing assembly (1).
15. Install 2 hex washer head tapping screws (2).

Tighten
Tighten the screws to 5.5 N·m (49 lb in).

16. Install the bearing retainer.
17. Install the lower bearing seat (3).
18. Install the lower bearing spring (2).
19. Install the lower spring retainer (1).
20. Install the retainer washer assembly (1).
21. Install the electrical BTSI actuator. Refer to Automatic Transmission Shift Lock Control Assemble - Off Vehicle .
22. Install the ignition switch assembly. Refer to Ignition Switch Assembly - Assemble - Off Vehicle .
23. Install the steering column housing assembly. Refer to Steering Column Jacket - Assemble - Off Vehicle .
24. Install the shift lever assembly. Refer to Shift Lever Replacement - On Vehicle .

## Steering Shaft, Lower Bearing, and Jacket - Assemble - Off Vehicle Floor Shift

1. Apply synthetic grease to the exposed shaft engagement areas (1). Install the lower steering shaft assembly (2) and the race and upper shaft assembly.
2. Install the lock plate (1).
3. Install the steering column housing shroud (2).
4. Install the steering column housing support assembly (3) with the dimmer switch rod (2) still connected.
5. Install the 4 torx head screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

6. Install the steering shaft assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

7. Install the adapter and bearing assembly (1).
8. Install 2 hex washer head tapping screws (2).

Tighten
Tighten the screws to 5.5 N·m (49 lb in).

9. Install the bearing retainer (1).
10. Install the lower bearing seat (3).
11. Install the lower bearing spring (2).
12. Install the lower spring retainer (1).
13. Install the retainer washer assembly (1).
14. Install the ignition switch assembly. Refer to Ignition Switch Assembly - Assemble - Off Vehicle .
15. Install the steering column housing assembly. Refer to Steering Column Jacket - Assemble - Off Vehicle .