For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 34730 Fuel Pressure Gauge

Important: Do Not attempt to repair sections of nylon fuel pipes. If the nylon fuel pipes are damaged, replace them.

1. Relieve the fuel system fuel pressure. Refer to Fuel Pressure Relief .
2. Drain the fuel tank (2). Refer to Fuel Tank Draining .
3. Raise the vehicle.
4. Remove the fuel tank (2) from the vehicle and place the fuel tank in a suitable work area. Refer to Fuel Tank Replacement .
5. Remove the fuel tank pressure sensor electrical sensor connector (2).