For 1990-2009 cars

#### Removal Procedure

1. Move the driver's seat forward.
2. Cut the carpet back under the driver's seat to expose the lateral accelerator switch.
3. Disconnect the electrical connector from the lateral accelerator switch.
4. Remove the two screws and the lateral accelerator switch.

#### Installation Procedure

1. Install the lateral accelerator switch with two screws.
2. Connect the electrical connector to the module.
3. Install the carpet.