For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the bulb/sockets from the lamp.
3. Remove the screws (3) that retain the lamp to the front bumper fascia (1).
4. Remove the front park/side marker lamp (2) from the fascia (1).

### Installation Procedure

1. Install the front park/side marker lamp (2) to the front bumper fascia (1).
2. Install the screws (3) in order to retain the lamp to the fascia (1).
3. Install the bulb/sockets to the lamp.
4. Lower the vehicle.