For 1990-2009 cars

## Exhaust Manifold Removal Left Side

1. Remove the left engine lift hook nut and bolt.
2. Remove the left engine lift hook.
3. Remove the exhaust manifold bolt and studs.
4. Remove the exhaust manifold.
5. Remove the exhaust manifold gasket.

## Exhaust Manifold Removal Right Side

1. Remove the EGR inlet pipe from the exhaust manifold.
2. Remove the EGR mounting bracket bolts.
3. Remove the EGR mounting bracket.
4. Remove the heated oxygen sensor lead.
5. Remove the fuel injector sight shield mounting bracket nuts.
6. Remove the fuel injector sight shield mounting bracket.
7. Remove the right engine lift hook nut and bolt.
8. Remove the right engine lift hook.
9. Remove the exhaust manifold studs.
10. Remove the exhaust manifold.
11. Remove the exhaust manifold gasket.