For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer Diagnostic System Check performed? | -- | Go to Step 2 | Go to Diagnostic System Check - Wiper/Washer
2 |

1. Turn the ignition switch to RUN.
2. Turn the wiper switch to OFF.
3. Disconnect the wiper/washer switch connector C202.

Do the wipers park?

--

Go to Step 3

Go to Step 4

3 | Replace the wiper/washer switch. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle . Is the replacement complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
4 | Measure the voltage from connector C202 (vehicle side), terminal E9 to ground with a DMM. Is the measurement greater than 1 V? | 1 V | Go to Step 6 | Go to Step 5
5 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
6 |

1. Reconnect the wiper/washer switch connector C202.
2. Disconnect wiper motor connector C1.
3. Measure the voltage from the wiper motor connector terminal F to ground with a DMM.

Is the measurement greater than 1 V?

1 V

Go to Step 8

Go to Step 7

7 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
8 | Repair the short circuit to battery voltage in CKT 94. Is the repair complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --