For 1990-2009 cars

### Removal Procedure

Important: Use tape on the tool surface to protect the paint on the antenna mast from damage.

1. Unscrew the antenna mast.
2. Remove the antenna mast from the antenna base.

### Installation Procedure

Important: Use tape on the tool surface to protect the paint on the antenna mast from damage.

1. Install the antenna mast to the antenna base.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Screw the antenna mast to the antenna base.

Tighten
Tighten the antenna mast to 5 N·m(44 lb in).