For 1990-2009 cars

1. Ensure that the window is in the full up position.
2. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Door Water Deflector Replacement .
4. Tighten the front run channel bolt in the center of the slot.
5. Loosen the fasteners that retain the window to the module sash.
6. Power the glass down 9 cm (3 in).
7. Slide the glass rearward in the sash fasteners.
8. Power the glass up.
9. Pry the glass up with a large flat screwdriver.
10. Tighten the fasteners that retain the window to the module sash.
11. Cycle the window up and down in order to inspect operation.
12. Install the water deflector. Refer to Door Water Deflector Replacement .
13. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .