For 1990-2009 cars

1. Insert the 2-3 accumulator valve bushing (345) into the valve body.
2. Insert the 2-3 accumulator valve (343) and the spring (344) into the valve body.
3. Install the bushing retainer (385).
4. Insert the 1-2 accumulator valve (341) and the spring (340) into the 1-2 accumulator bushing (342).
5. Insert the 1-2 accumulator bushing plug (339) and the plug retainer (338) into the 1-2 accumulator bushing (342).
6. Insert the 1-2 accumulator valve assembly into the valve body.
7. Install the 1-2 accumulator bushing retainer (385).
8. Insert the 3-4 accumulator valve bushing (352) into the valve body.
9. Insert the 3-4 accumulator valve (350) and the spring (351) into the valve body.
10. Install the bushing retainer (385).
11. Install the 1-2 accumulator valve (347) and the spring (348) into the 1-2 accumulator bushing (349).
12. Insert the 1-2 accumulator bushing plug (346) and the plug retainer (338) into the 1-2 accumulator bushing (349).
13. Insert the 1-2 accumulator valve assembly into the valve body.
14. Install the 1-2 accumulator bushing retainer (385).
15. Install the 2-3 shift valve (357) into the valve body.
16. Assemble the 3-2 manual downshift valve (356) and the spring (355).
17. Insert the bore plug (354) into the valve body.
18. Install the bore plug retainer (353).
19. Install the 3-4 shift valve (362) into the valve body.
20. Assemble the 4-3 manual downshift valve (360) and the spring (361).
21. Insert the bore plug (359) into the valve body.
22. Install the bore plug retainer (358).
23. Insert a new seal (316) onto the 2-3 shift solenoid valve (315).
24. Install the 2-3 shift solenoid valve (315) into the valve body.
25. Install the solenoid valve retainer (314).
26. Assemble the reverse boost valve (367) and the spring (365).
27. Install the boost valve bore plug (364).
28. Install the coiled spring pin (363).
29. Assemble the forward servo boost valve (367) and the valve spring (366).
30. Install the forward boost valve retainer pin (363).
31. Install the reverse boost valve (310), the springs (311, 312), and the pressure regulator valve (313) into the valve body.
32. Assemble the reverse boost valve bushing (309) and the retainer (308).
33. Insert the reverse boost spring (307) into the valve body.
34. Insert the pressure regulator retainer (306).
35. Install the spring (305), the line boost valve (304), and the bore plug (303) into the valve body.
36. Install the line boost valve retainer (302).
37. Install the valve spring (317) and the 1-2 shift valve (318) into the 1-2 shift valve body.
38. Insert the seal (316) onto the 1-2 shift solenoid valve (315).
39. Insert the shift solenoid valve (315) into the valve body.
40. Install the shift solenoid valve retainer (314).
41. Insert the valve spring (323), the valve seat (322), and the valve (321) into the oil pump pressure relief valve body.
42. Insert the pressure relief bushing (320) into the valve body.
43. Install the bushing retaining pin (319)
44. Affix new seals (326, 327) onto the PWM solenoid valve assembly (325).
45. Insert the solenoid valve (325) into the valve body.
46. Install the retainer (324) into the PWM solenoid valve assembly.
47. Insert the isolator spring (333) and the valve (334) into the valve body.
48. Insert the torque converter clutch (TCC) regulator valve (332) and the spring (331) into the valve sleeve (384).
49. Insert the valve sleeve assembly into the valve body.
50. Insert the TCC regulator valve retainer (383).
51. Insert the TCC valve (335) into the valve body.
52. Install a new seal (316) onto the TCC solenoid valve (315).
53. Insert the solenoid valve (315) into the valve body.
54. Install the solenoid valve retainer (314).