For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the RUN position.
2. Place the gear selector lever in the PARK position.

The backup lights are off.

• | Backup Lamps Always On

• | Backup Lamps Always On

2 | Place the gear selector lever in the REVERSE position. | The backup lights are on. | Backup Lamps Inoperative
3 | Place the gear selector lever in the NEUTRAL position. | The backup lights are off. |

• | Backup Lamps Always On

• | Backup Lamps Always On

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.