For 1990-2009 cars

### Removal Procedure

1. Remove the fuel filler door. Refer to Fuel Tank Filler Door Replacement .
2. Remove the fuel filler door latch. Refer to Fuel Filler Door Release Replacement.
3. Disconnect the electrical connector (1).
4. Remove the bolts (3).
5. Remove the fuel filler door latch actuator (2) by pulling the cable (4) and the grommet (5) through the hole in the body.

### Installation Procedure

1. Install the fuel filler door latch actuator (2) by feeding the cable (4) through the hole in the body. Ensure that the cable is in the fuel filler pocket area.

Important: Fully seat the grommet.

2. Press the grommet (5) into the hole in the body.
3. Connect the electrical connector (1).
4. Install the bolts (3).
5. Install the fuel filler door latch. Refer to Fuel Filler Door Release Replacement.
6. Install the fuel filler door. Refer to Fuel Tank Filler Door Replacement .