For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
RH IP Fuse Block | Under the right side of the IP, near the rear of the IP compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
RH Underhood Fuse Block | Center rear of the engine compartment, near the cowl | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Sunroof Actuator | In the center of the passenger compartment, in the rear of the headliner | Power Roof Systems Component Views in Roof | Power Roof Systems Connector End Views in Roof
Sunroof Control Module | In the center of the passenger compartment, in the rear of the headliner | Power Roof Systems Component Views in Roof | Power Roof Systems Connector End Views in Roof
Sunroof Switch | Center of overhead console | Power Roof Systems Component Views in Roof | Power Roof Systems Connector End Views in Roof
C221 (3 cavities) | Body harness to the sunroof harness, right hand of the passenger compartment, on the top of the front pillar | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G201 | In the right front of the passenger compartment, behind the right kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P101 | In the right rear of the engine compartment, near the right hand strut tower | Harness Routing Views in Wiring Systems | --
P500 | On the front of the left hand door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S203 | In the body harness, approximately 43.5 cm (17.1 in) from the IP fuse block | Harness Routing Views in Wiring Systems | --
S308 | In the body harness, approximately 33 cm (13 in) from the G201 breakout | Harness Routing Views in Wiring Systems | --
S501 | In the body harness, approximately 43 cm (16.9 in) from P500 | Harness Routing Views in Wiring Systems | --