For 1990-2009 cars

Important: Do not remove any of the bore plugs unless inspection indicates that replacement is necessary.

1. Remove the manual valve (404).
2. Remove the cylinder (421) and the seal (422) for the 3-4 accumulator piston.
3. Remove the outer spring (423), middle spring (424), and inner spring (425) for the 3-4 accumulator piston.
4. Remove the pin (426) for the 3-4 accumulator piston.