For 1990-2009 cars

#### Tools Required

J 29862 Camber Adjustment Tool

1. Loosen the strut to knuckle mounting nuts.

Tighten
Tighten the strut to knuckle mounting bolts, usingJ 29862 , to 190 N·m (140 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Refer to Wheel Alignment Specifications .
3. Remove J 29862 .