For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

• | Adjust the tire pressure to specifications.

• | Inspect for proper trim heights.

• | Inspect the brakes for drag.

Does the vehicle still lead or pull?

--

Go to Step 2

System OK

2 | Road test the vehicle. Does the vehicle still lead or pull? | -- | Go to Step 3 | System OK
3 | Cross switch the front tire and wheel assemblies. Does the vehicle still lead or pull? | -- | Go to Step 4 | System OK
4 | Road test the vehicle. Does the vehicle still lead or pull in the same direction? | -- | Go to Step 5 | Go to Step 9
5 | Inspect front wheel alignment. Adjust front wheels to proper alignment. Does the vehicle still lead or pull in the same direction? | -- | Go to Step 5 | Go to Step 8
6 | Inspect caster-camber-toe for proper alignment. Is the caster-camber-toe improperly aligned? | -- | Go to Step 7 | Go to Step 8
7 | Align the caster-camber-toe. Does the vehicle still lead or pull? | -- | Go to Step 8 | System OK
8 | Road test the vehicle. Does the vehicle lead or pull in the opposite direction? | -- | Go to Step 9 | System OK
9 | Swap the left front tire and wheel assemblies with the left rear tire and wheel assemblies. Does the vehicle still lead or pull in the opposite direction? | -- | Go to Step 10 | System OK
10 | Swap the right front tire and wheel assemblies with the right rear tire and wheel assemblies. Does the vehicle still lead or pull in the opposite direction? | -- | Go to Step 11 | System OK
11 | Change the camber setting. Does the vehicle still lead or pull? | -- | Go to Step 12 | System OK
12 |

• | If the vehicle leads or pulls to the left, add an additional -0.5 degree camber on the left and +0.5 degree camber on the right.

• | If the vehicle leads or pulls to the right, add an additional +0.5 degree camber on the left and -0.5 degree camber on the right.

• | Does the vehicle still lead or pull?

--

Go to Step 13

System OK

13 |

• | If the vehicle leads or pulls to the left, increase (-) camber on the left and (+) camber on the right until pull is eliminated.

• | If the vehicle leads or pulls to the right, increase (+) camber on the left and (-) camber on the right until pull is eliminated.

• | Does the vehicle still pull?

--

--

System OK