For 1990-2009 cars

### Removal Procedure

1. Remove the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the panel lights/twilight sentinel/traction control switch (4) fasteners.
3. Pull rearward on the switch assembly (4) in order to remove the switch.

### Installation Procedure

1. Install the panel lights/twilight sentinel/traction control switch (4).
2. Install the fasteners.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the fasteners to 1.9 N·m (17 lb in)

3. Install the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .