For 1990-2009 cars

• | If abnormal noise exists in the rear end, inspect for the following conditions:

- | The exhaust system contacts the underbody

- | Worn or damaged dual axis ball joint

- | Damaged strut or mountings

- | Worn or damaged rear toe link

- | Worn control arm bushings

- | Loose stabilizer shaft

- | Loose wheel nuts

- | Loose suspension mounting bolts

- | Noisy wheel covers

- | Tire noise

• | Inspect for diagnostic trouble codes in the computer command ride system.