For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 25034-C Pulley Remover

1. Remove the pump drive belts. Refer to Drive Belt Replacement in Engine Mechanical.
2. Remove the pump from the engine. Refer to Power Steering Pump Replacement .
3. Use the J 25034-C in order to remove the pulley from the pump.

### Installation Procedure

#### Tools Required

J 25033-C Pulley Installer

1. Use the J 25033-C in order to install the pulley onto the pump.
2. Axial tolerance of the pulley on the pump shaft is -0.25 mm to 0.25 mm (-0.010 in to 0.010 in).
3. Install the pump to the engine. Refer to Power Steering Pump Replacement
4. Install the pump drive belt. Refer to Drive Belt Replacement in Engine Mechanical.
5. Bleed the power steering system.
6. Inspect the system for leaks.