For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 36850 Transjel

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the case side cover. Refer to Control Valve Body Cover Replacement
3. Remove the wiring harness as necessary.
4. Remove the oil pump. Refer to Oil Pump Replacement
5. Remove the valve body to channel plate bolts.
6. Remove the valve body. Leave the spacer plate with the transmission.
7. Remove the spacer plate and the spacer plate gasket, as necessary.
8. Remove the solenoid screens.

### Installation Procedure

Notice: The assembly of some components will require the use of an assembly lube. Always use J 36850 Transjel™ or petroleum jelly during assembly. Greases other than the recommended assembly lube will change the transmission fluid characteristics and cause undesirable shift conditions and/or filter clogging.

1. In order to retain the checkballs in their proper locations, use the J 36850 or equivalent petroleum jelly.
2. Install the solenoid screens, if necessary.
3. Install the spacer plate and the spacer plate gasket, as necessary.
4. Install the valve body and the valve body gasket.
5. Install the valve body to channel plate bolts to specifications.

Notice: Use a torque wrench to tighten the pump to valve body bolts. Do not exceed the torque specifications.

Notice: Install all the valve body bolts, then torque the bolts in a spiral pattern starting from the center, as shown. If you torque the bolts at random, you may distort the valve bores. This will inhibit valve operation.

Important: Do not use impact type tools on the valve body or the pump assembly.

6. Install the oil pump. Refer to Oil Pump Replacement
7. Install the wiring harness.
8. Install the case side cover. Refer to Control Valve Body Cover Replacement
9. Connect the negative battery cable.
10. Adjust the oil level.