For 1990-2009 cars

## Lumbar Support Inoperative Oldsmobile w/AL2 LH

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Lumbar Support System Check? | -- | Go to Step 2 | Go to Lumbar Support System Check
2 | Backprobe connector C312 with a DMM from cavity A (ORN) to ground. Is the voltage within the specified range? | 10-15 V | Go to Step 3 | Go to Step 4
3 | Backprobe connector C312 with a DMM from cavity A (ORN) to cavity B (BLK). Is the voltage within the specified range? | 10-15 V | Go to Step 6 | Go to Step 5
4 | Repair the open in CKT 1340 (ORN) between S227 and C312. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
5 | Repair the open in CKT 1250 (BLK) between C312 and S218. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
6 |

1. Hold the LH lumbar switch in the INFLATE position.
2. Backprobe with a DMM from the LH lumbar air pump connector power cavity (RED) to connector C312 cavity B (BLK).

Is the voltage within the specified range?

10-15 V

Go to Step 7

Go to Step 8

7 | Replace the LH lumbar air pump. Is the repair complete? | -- | Go to Lumbar Support System Check | --
8 | Replace the LH lumbar switch. Is the repair complete? | -- | Go to Lumbar Support System Check | --

## Lumbar Support Inoperative Pontiac w/AL7

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Lumbar Support System Check? | -- | Go to Step 2 | Go to Lumbar Support System Check
2 | Backprobe the console seat switch connector C1 with a DMM from cavity C (ORN) to ground. Is the voltage within the specified range? | 10-15 V | Go to Step 3 | Go to Step 11
3 |

1. Disconnect the seat air control module connector.
2. Connect a DMM from the seat air control module connector cavity F (ORN) to ground.

Is the voltage within the specified range?

10-15 V

Go to Step 4

Go to Step 12

4 |

1. Connect a DMM from the seat air control module connector cavity F (ORN) to cavity B (BLK).
2. Connect a DMM from the seat air control module connector cavity F (ORN) to cavity E (BLK).

Is the voltage within the specified range for both ground cavities?

10-15 V

Go to Step 5

Go to Step 13

5 |

1. Connect a DMM from battery positive voltage (B+) to the seat air control module connector cavity A (BLK).
2. Move the seat select switch to operate the inoperative seat.

Is the voltage within the specified range with the switch operated?

10-15 V

Go to Step 6

Go to Step 14

6 |

1. Connect a DMM from the seat air control module connector cavity D (WHT) to ground.
2. Operate any of the inflate switches.

Is the voltage within the specified range with the switches operated?

10-15 V

Go to Step 7

Go to Step 15

7 |

1. Connect a DMM from the seat air control module connector cavity H (GRY) to ground.
2. Operate any of the deflate switches.

Is the voltage within the specified range with the switches operated?

10-15 V

Go to Step 8

Go to Step 16

8 |

1. Backprobe the seat air pump connector with a DMM from cavity A (TAN) to ground.
2. Operate any of the inflate switches.

Is the voltage within the specified range with the switches operated?

10-15 V

Go to Step 9

Go to Step 18

9 |

1. Backprobe the seat air pump connector with a DMM from cavity B (PPL) to ground.
2. Operate any of the deflate switches.

Is the voltage within the specified range with the switches operated?

--

Go to Step 10

Go to Step 19

10 | Replace the seat air pump. Is the repair complete? | -- | Go to Lumbar Support System Check | --
11 | Repair the open in CKT 640 (ORN) between S237 and the console seat switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
12 | Repair the open in CKT 1340 (ORN) between S227 and the seat air control module. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
13 | Repair the open in CKT 1250 (BLK) between the seat air control module and S362. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
14 | Test for an open in CKT 769 (BLK) between the console seat switch and the seat air control module. Refer to Testing for Continuity in Wiring Systems. Is CKT 769 OK? | -- | Go to Step 17 | Go to Step 21
15 | Test for an open or short to ground in CKT 766 (WHT) between the console seat switch and the seat air control module. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 766 OK? | -- | Go to Step 17 | Go to Step 21
16 | Test for an open or short to ground in CKT 764 (GRY) between the console seat switch and the seat air control module. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 764 OK? | -- | Go to Step 17 | Go to Step 21
17 | Replace the console seat switch. Is the repair complete? | -- | Go to Lumbar Support System Check | --
18 | Test for an open or short to ground in CKT 768 (TAN) between the seat air control module and the seat air pump. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 768 OK? | -- | Go to Step 20 | Go to Step 21
19 | Test for an open or short to ground in CKT 767 (PPL) between the seat air control module and the seat air pump. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 767 OK? | -- | Go to Step 20 | Go to Step 21
20 | Replace the seat air control module. Is the repair complete? | -- | Go to Lumbar Support System Check | --
21 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --

## Lumbar Support Inoperative Oldsmobile w/AL2 RH

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Lumbar Support System Check? | -- | Go to Step 2 | Go to Lumbar Support System Check
2 | Backprobe connector C313 with a DMM from cavity A (ORN) to ground. Is the voltage within the specified range? | 10-15 V | Go to Step 3 | Go to Step 4
3 | Backprobe connector C313 with a DMM from cavity A (ORN) to cavity B (BLK). Is the voltage within the specified range? | 10-15 V | Go to Step 6 | Go to Step 5
4 | Repair the open in CKT 1340 (ORN) between S227 and C313. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
5 | Repair the open in CKT 1450 (BLK) between C313 and S307. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Lumbar Support System Check | --
6 |

1. Hold the RH lumbar switch in the inflate position.
2. Backprobe with a DMM from the RH lumbar air pump connector power cavity (RED) to connector C313 cavity B (BLK).

Is the voltage within the specified range?

10-15 V

Go to Step 7

Go to Step 8

7 | Replace the RH lumbar air pump. Is the repair complete? | -- | Go to Lumbar Support System Check | --
8 | Replace the RH lumbar switch. Is the repair complete? | -- | Go to Lumbar Support System Check | --