For 1990-2009 cars

Condition | Causes
--- | ---
The steering wheel is loose. |

• | Excessive clearance exists between the pivot pin diameters and the holes in the support or in the housing.

• | The anti-lash spring in the spheres is damaged.

• | The anti-lash spring in the spheres is missing.

• | The upper bearing is not seated in the housing.

• | The inner race seal is missing from the upper bearing.

• | The support screws are loose.

• | The bearing preload spring is missing.

• | The bearing preload spring is broken.