For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Briefly press each of the left seat switches in the following directions:

• | Front vertical: UP

• | Front vertical: DOWN

• | Rear vertical: UP

• | Rear vertical: DOWN

• | Entire seat: UP

• | Entire seat: DOWN

• | Forward/back: FORWARD

• | Forward/back: BACK

• | Recline: FORWARD

• | Recline: BACK

The left seat moves in the selected direction.

• | Power Seat Inoperative

• | Power Seat Does Not Recline

• | Power Seat Inoperative in One Direction

2 | Momentarily press the DRIVER-1 switch. | The left seat and both of the outside rear view mirrors move to the DRIVER-1 programmed settings, and a single beep is heard. |

• | Memory Seat Feature Inoperative

• | Memory Seat For/Rearward Does Not Set or Recall

• | Memory Seat Forward Tilt Does Not Set or Recall

• | Memory Seat Rearward Tilt Does Not Set or Recall

3 | Momentarily press the DRIVER-2 switch. | The left seat and both of the outside rear view mirrors move to the DRIVER-2 programmed settings, and a single beep is heard. |

• | Memory Seat Feature Inoperative

• | Memory Seat For/Rearward Does Not Set or Recall

• | Memory Seat Forward Tilt Does Not Set or Recall

• | Memory Seat Rearward Tilt Does Not Set or Recall

4 |

1. Manually move the left seat fully forward and up.
2. Press SET MEMORY, followed by the DRIVER-1 switch within 5 seconds.
3. Simultaneously press the DRIVER-1 and DRIVER-2 switches.
4. Momentarily press the DRIVER-1 switch.
5. Repeat the above steps for the DRIVER-2 switch.

1. The left seat moves fully forward and up.
2. A beep is heard to acknowledge that the DRIVER-1 settings are stored for fully forward and up.
3. The left seat moves to the EASY EXIT position (fully down and fully back).
4. The left seat returns to the fully forward and up position.
5. The DRIVER-2 functions properly.

• | Power Seats - Memory Switch Inoperative

• | Memory Seat Feature Inoperative

5 |

1. Move the seat in all directions.
2. Press the keyless entry transmitter UNLOCK button.

There are 4 personalized options for the keyless entry recall function. Refer to Circuit Operation for the personalized options.

Refer to Remote Keyless Entry System Check in Keyless Entry.

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.