For 1990-2009 cars

1. Use a small screwdriver in order to align the teeth of the input clutch plate assembly and the third clutch plate assembly. This will ease installation of the sprag clutch assembly.

Important: Make sure that the sprag clutch assembly is fully seated into the housing.

2. Insert the combined input sprag clutch (665), third sprag clutch (653) and input sun gear (668) assembly into the input clutch housing assembly (632).