For 1990-2009 cars

1. Assemble the transaxle oil dam (27) into the case.
2. Assemble the manual valve link and spring assembly (402, 403) into the manual shift detent lever (802).
3. Pull back the manual valve spring (403) and connect the manual valve link (402) to the manual valve (404).
4. Assemble the manual shift detent assembly (804), and bolt (805).

Tighten
Tighten the bolt to 11 N·m (97 lb in).

Refer to Fastener Notice .

5. Carefully install the input speed sensor (440) into the case cover (400).
6. Install the input speed sensor clip (441) into the case cover (400).