For 1990-2009 cars

#### Tools Required

J 33049 Camshaft Bearing Installer

1. Select the camshaft bearings.
2. Use the following procedure to install the camshaft bearings:

2.1. | Assemble J 33049 according to the manufacturer's instructions.

2.2. | Place the bearing on the tool.

| Notice: Severe engine damage may result if the oil holes are not correctly aligned.

2.3. | Index the bearing oil holes with the engine block oil passages.