For 1990-2009 cars

## Front Bumper Fascia Air Deflector Replacement Buick

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the screws that retain the lower air deflector (4) to the front bumper fascia (1).
3. Remove the lower air deflector (4).

### Installation Procedure

1. Install the lower air deflector (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fasteners (5) in order to retain the lower air deflector (4) to the front bumper fascia.

Tighten
Tighten the fasteners to 2.8 N·m (25 lb in).

3. Lower the vehicle.

## Front Bumper Fascia Air Deflector Replacement Oldsmobile

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the bolts (4) that attach the lower air deflector (3) to the fascia supports (2,6).
3. Remove the bolts (4) that attach the lower air deflector to the front bumper fascia (1).

### Installation Procedure

1. Install the bolts (4) in order to connect the lower air deflector (3) to the front bumper fascia (1).
2. Install the bolts (4) in order to attach the lower air deflector to the fascia supports (2,6).
3. Lower the vehicle.

## Front Bumper Fascia Air Deflector Replacement Pontiac

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the screws (5) that retain the lower air deflector (4).
3. Remove the lower air deflector (4).

### Installation Procedure

1. Install the lower air deflector (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fasteners (5) in order to retain the lower air deflector (4).

Tighten
Tighten the fasteners to 2.8 N·m (25 lb in).

3. Lower the vehicle.