For 1990-2009 cars

#### Tools Required

J 35628-A Vats/Pass Interrogator Tester

Important: When servicing the PASS-Key® II system, obtain all the vehicle ignition keys. Verify the key code values with the J 35628-A .

1. In order to copy a PASS-Key® II ignition key, determine the necessary key code or resistance value.
2. Determine the master ignition key code using the J 35628-A as outlined in the following procedure:

| Important: Disconnect the tool wiring connectors.

2.1. | Turn ON the J 35628-A .

2.2. | Insert the key into the tool lock cylinder.

2.3. | Note the measured key code of the master ignition key as displayed on the key code reader.

2.4. | Obtain a key blank matching the key code.

2.5. | Cut the key blank to match the original key.