For 1990-2009 cars

Condition | Causes
--- | ---
A high lock effort exists. |

• | The lock cylinder is damaged.

• | The ignition switch is damaged.

• | A rack preload spring is broken.

• | A rack preload spring is broken.

• | Burrs exist on the following items:

- | The sector

- | The rack

- | The housing

- | The support

- | The actuator rod coupling

• | The sector shaft is bent.

• | A rack is damaged.

• | The housing is extreme misaligned to the cover.

• | A coupling slot in the rack is distorted.

• | An actuator rod is damaged.

• | The ignition switch mounting bracket is bent.

• | An actuator rod is restricted.

• | The key cut is damaged.

• | The key cut is incorrect.

• | The park lock cable is incorrectly adjusted.

• | The park lock components are damaged.