For 1990-2009 cars

## Front Bumper Fascia Molding Replacement Buick

### Removal Procedure

1. Gently peel the molding (2) away from the fascia (1).
2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive tape on the new molding (2).
2. Apply the molding to the fascia (1).

## Front Bumper Fascia Molding Replacement Oldsmobile

### Removal Procedure

1. Gently peel the molding (2) away from the fascia (1).
2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive tape on the new molding (2).
2. Apply the molding (2) to the fascia (1).

## Front Bumper Fascia Molding Replacement Pontiac

### Removal Procedure

1. Gently peel the molding (2) away from the fascia (1).
2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive tape on the new molding (2).
2. Apply the molding to the fascia (1).