For 1990-2009 cars

## Rocker Panel Molding Replacement Buick

### Removal Procedure

1. Remove the screws (2).
2. Slide the molding (1) toward the rear of the vehicle in order to disengage the fasteners, if equipped.
3. Remove the rocker panel molding (1).

### Installation Procedure

1. Position the rocker panel molding (1).
2. Secure the molding (1) by striking firmly at each clip location, if equipped.
3. Install the screws (2).

## Rocker Panel Molding Replacement Regency

### Removal Procedure

1. Remove the screws (1,2).
2. Slide the molding (3) toward the rear of the vehicle in order to disengage the fasteners, if equipped.
3. Remove the rocker panel molding (3).

### Installation Procedure

1. Position the rocker panel molding (3).
2. Secure the molding by striking firmly at each clip location, if equipped.
3. Install the screws (1,2).

## Rocker Panel Molding Replacement Oldsmobile 88/LSS

### Removal Procedure

1. Remove the screws (1,4,5).
2. Slide the molding toward the rear of the vehicle in order to disengage the fasteners, if equipped.
3. Remove the rocker panel molding (2).

### Installation Procedure

1. Position the rocker panel molding (2).
2. Secure the molding, if equipped, by striking firmly at each clip location.
3. Install the screws (1,4,5).

## Rocker Panel Molding Replacement Bonneville SSE/SSEi

### Removal Procedure

1. Remove the screws (2,3).
2. Slide the molding toward the rear of vehicle in order to disengage the fasteners, if equipped.
3. Remove the rocker panel molding (1).

### Installation Procedure

1. Position the rocker panel molding (1).
2. Secure the molding by striking firmly at each clip location, if equipped.
3. Install the screws (2,3).

## Rocker Panel Molding Replacement Bonneville SE

### Removal Procedure

1. Remove the screws (2).
2. Slide the molding toward the rear of the vehicle in order to disengage fasteners, if equipped.
3. Remove the rocker panel molding (1).

### Installation Procedure

1. Position the rocker panel molding (1).
2. Secure the molding (1) by striking firmly at each clip location, if equipped.
3. Install the screws (2).