For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Accelerator Control Cable Bracket Bolt | 16 | 12 | --
Balance Shaft Driven Gear Bolt | 22 + 70° | 16 + 70° | --
Balance Shaft Retainer Bolt | 30 | 22 | --
Camshaft Position Sensor Bolt | 10 | -- | 89
Camshaft Sprocket Bolt | 100 + 90° | 74 + 90° | --
Camshaft Thrust Plate Bolt | 15 | 11 | --
Canister Purge Solenoid Valve Bracket Bolt (VIN K) | 50 | 37 | --
Canister Purge Vacuum Switch Bolt (VIN K) | 50 | 37 | --
Connecting Rod Cap Bolt | 27 + 50° | 20 + 50° | --
Crankshaft Balancer Bolt | 150 + 76° | 111 + 76° | --
Crankshaft Main Bearing Cap Bolt | 40 + 110° | 30 + 110° | --
Crankshaft Main Bearing Cap Bolt (Side) | 15 + 45° | 11 + 45° | --
Crankshaft Position Sensor Stud | 30 | 22 | --
Crankshaft Rear Oil Seal Housing Bolt | 15 + 50° | 11 + 50° | --
Cylinder Head Bolt | 50 + 120° | 37 + 120° | --
Drive Belt Tensioner Bracket Bolt/Nut | 50 | 37 | --
Drive Belt Tensioner Bracket Stud | 6 | -- | 53
EGR Valve Adapter Bolt | 50 | 37 | --
EGR Valve Inlet Pipe Bolt | 29 | 21 | --
EGR Valve Nut | 29 | 21 | --
EGR Valve Outlet Pipe Bolt/Nut | 29 | 21 | --
Engine Block Coolant Drain Plug (VIN 1) | 18 | 13 | --
Engine Block Coolant Drain Plug (VIN K) | 30 | 22 | --
Engine Block Oil Gallery Plug | 30 | 22 | --
Engine Coolant Temperature Sensor | 25 | 18 | --
Engine Flywheel Bolt | 15 + 50° | 11 + 50° | --
Engine Front Cover Bolt/Stud | 20 + 40° | 15 + 40° | --
Engine Lift Bracket Bolt/Nut/Stud | 30 | 22 | --
Engine Mount Nut, Lower | 78 | 58 | --
Engine Mount Nut, Upper | 78 | 58 | --
Engine Oil Pressure Indicator Switch | 16 | 12 | --
Exhaust Crossover Heat Shield Nut | 20 | 15 | --
Exhaust Crossover Pipe Bolt/Stud | 20 | 15 | --
Exhaust Manifold Bolt/Nut | 30 | 22 | --
Exhaust Manifold Heat Shield Nut | 20 | 15 | --
Exhaust Manifold Stud (Inner) | 30 | 22 | --
Exhaust Manifold Stud (Outer) | 10 | -- | 89
Fuel Injector Rail Nut | 10 | -- | 89
Fuel Injector Rail Stud | 25 | 18 | --
Fuel Injector Sight Shield Bracket Nut | 30 | 22 | --
Generator Brace Bracket Bolt | 50 | 37 | --
Heated Oxygen Sensor | 42 | 31 | --
ICM Bolt (VIN 1) | 30 | 22 | --
ICM Nut | 50 | 37 | --
ICM Stud (VIN K) | 6 | -- | 53
ICM Wiring Harness Bolt | 2 | -- | 18
Idler Pulley Bolt | 50 | 37 | --
Idler Pulley Bracket Bolt | 30 | 22 | --
Lower Intake Manifold Bolt | 15 | 11 | --
MAP Sensor Bolt (VIN 1) | 3 | -- | 27
MAP Sensor Bracket Bolt (VIN 1) | 30 | 22 | --
Oil Cooler Adapter Connector | 50 | 37 | --
Oil Filter | 30 | 22 | --
Oil Filter Adapter Bolt | 15 + 50° | 11 + 50° | --
Oil Level Indicator Switch | 20 | 15 | --
Oil Level Indicator Tube Nut | 19 | 14 | --
Oil Pan Bolt | 14 | -- | 125
Oil Pan Drain Plug | 30 | 22 | --
Oil Pump Cover Screw | 11 | -- | 98
Oil Pump Screen Bolt | 15 | 11 | --
Power Brake Booster Heat Shield Nut | 20 | 15 | --
Spark Plug | 27 | 20 | --
Starter Motor Heat Shield Bolt | 30 | 22 | --
Supercharger Bolt/Stud (VIN 1) | 23 | 17 | --
Supercharger Bypass Valve and Fuel Pressure Regulator Valve Harness Bolt (VIN 1) | 10 | -- | 89
Supercharger Bypass Valve Nut (VIN 1) | 8 | -- | 71
Throttle Body Nut | 10 | -- | 89
Throttle Body Support Bolt (VIN K) | 10 | -- | 89
Timing Chain Dampener Bolt | 22 | 16 | --
Upper Intake Manifold Bolt (VIN K) | 10 | -- | 89
Valve Lifter Guide Retainer Bolt | 30 | 22 | --
Valve Rocker Arm Bolt | 15 + 90° | 11 + 90° | --
Valve Rocker Arm Cover Bolt | 10 | -- | 89
Water Outlet Bolt | 27 | 20 | --
Water Pump Bolt | 15 + 80° | 11 + 80° | --
Water Pump Pulley Bolt | 13 | -- | 116
Wiring Harness Shield Bolt/Nut | 10 | -- | 89