For 1990-2009 cars

Indicator | Bulbs to Check
--- | ---
Important: When replacing a bulb, ensure that you replace the bulb with the same type. If you use the incorrect bulb, the driver information center (DIC) will continue to display a bulb outage. If the driver information center (DIC) displays bulb indicator outages, use the following chart before proceeding with the diagnosis in order to determine if a bulb is burnt out. Verify the proper bulb type.
The high beam indicator lights. | The 2 high beam bulbs
The low beam indicator lights. | The 2 low beam bulbs
The park lamp lights. |

• | The LH park/turn bulb

• | The LH side marker bulb

• | The RH park/turn bulb

• | The RH side marker bulb

The turn lamp lights. |

• | The LH front turn signal bulb.

• | The RH front turn signal bulb.

• | The LH rear turn signal bulb.

• | The RH rear turn signal bulb.

The taillamp indicator lights. |

• | The 2 left tail bulbs

• | The 2 right tail bulbs

• | The 2 licence bulbs

• | The 4 tail/turn/stop bulbs

• | The LH rear side marker bulb

• | The RH rear side marker bulb

The backup indicator lights. | The 2 backup bulbs
The brake lamp indicator comes on |

• | The 4 stop/turn tail bulbs

• | The 1 CHMSL bulb

The taillamp indicator and the brake indicator light at the same time. |

• | The 2 LH stop/turn/tail bulbs

• | The 2 right stop/turn/tail/bulbs