For 1990-2009 cars

### Removal Procedure

1. Raise the head restraint (1) to the full up position.
2. Disengage the lock by inserting a piece of wire or a paper clip into the hole in the front of the headrest guide.
3. Pull the head restraint out of the guide.

### Installation Procedure

1. Insert the head restraint into the head restraint guides (1).

Push the head restraint to the full-down position.

2. Verify that the lock springs engage by pulling upward on the head restraint.