For 1990-2009 cars

#### Tools Required

J 34094-A Thermal Element Height Gauge

1. Remove the thermo element plate pins (120).
2. Remove the thermo element (121) and the thermo element plate (122).
3. Use J 34094-A in order to set the height of the thermo element plate center pin (123).
4. Install the thermo element plate (122).
5. Use J 34094-A in order to set the height of the thermo element plate pin (120) that is farthest from the accumulators.
6. Use J 34094-A in order to set the height of the second thermo element plate pin (120).
7. Carefully install the thermo element (121) between the two thermo element plate pins (120).
8. The V in the thermo element (121) must contact the thermo element plate (123).