For 1990-2009 cars

If hard steering exists, inspect for the following conditions:

• | Magnasteer™ system malfunction (at low speeds).

• | Intermediate shaft coupling damaged or worn

• | Tight steering column bearings

• | Sticking flow control valve

• | Insufficient pump pressure

• | Air in power steering system

• | Low fluid level

• | Excessive internal pump leakage

• | Excessive internal rack and pinion leakage