For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Inspect CKT 32 (YEL) between S223 and the underhood lamp for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 5 | Go to Step 3
3 | Inspect CKT 1150 (BLK) between S128 and the underhood lamp for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 5 | Go to Step 4
4 | Replace the vanity mirror. Refer to Vanity Mirror Lamp Replacement in Interior Trim. Is the repair complete? | -- | Go to Interior Lamps System Check | --
5 | Repair or replace the faulty circuit. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --