For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .
2. Rotate the throttle lever.
3. Remove the cruise control cable (1) from the accelerator controls cable bracket (2).
4. Disconnect the accelerator control cable (2) from the accelerator controls cable bracket (1).
5. (VIN K Only) Remove the wiring harness clip (1) from accelerator controls cable bracket (3).
6. Remove the two bolts from the accelerator controls cable bracket.

### Installation Procedure

Notice: Do not route flexible components (hoses, wires, conduits, etc.) within 50 mm (2 in) of moving parts unless flexible components can be securely fastened. This is necessary in order to prevent possible interference and damage to the component.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the two bolts to the accelerator controls cable bracket.

Tighten
Tighten the bolts to 16 N·m (12 lb ft).

2. (VIN K Only) Install wiring harness clip (1) to the accelerator controls cable bracket (3).
3. Install the accelerator controls cable (2) to the accelerator controls cable bracket (1).
4. Install the cruise control cable (1) to the accelerator controls cable bracket (2).

Important: The throttle should operate freely, without binding, between full closed and wide open throttle.

5. Check for complete throttle opening and closing positions by operating the accelerator pedal. Also check for poor carpet fit under the accelerator pedal.
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .

Tighten
(VIN 1 Only) Tighten the bolt to 2 N·m (18 lb in).