For 1990-2009 cars

## Front Fender Body Side Molding Replacement Buick

### Removal Procedure

1. Remove the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.
2. Remove the 2 nuts (2).

### Installation Procedure

1. Install the following components:

• | The molding (3)

• | The 2 nuts (2

2. Install the front wheelhouse panel. Refer to Wheelhouse Panel Replacement .

## Front Fender Body Side Molding Replacement Regency

### Removal Procedure

1. Remove the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.
2. Remove the screws (2) that retain the fender molding (1) at the wheel opening.
3. Remove the nuts (3) that retain the fender molding (1) to the fender.
4. Remove the fender molding (1).

### Installation Procedure

1. Install the fender molding (1).
2. Install the nuts (3) in order to retain the fender molding (1) to the fender.
3. Install the screws (2) in order to retain the fender molding (1) at the wheel opening.
4. Install the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.

## Front Fender Body Side Molding Replacement 88/LSS

### Removal Procedure

1. Remove the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.
2. Remove the screws (7) that retain the fender molding (6) to the fender.
3. Remove the fender molding (6).

### Installation Procedure

1. Install the fender molding (6).
2. Install the screws (7) in order to retain the fender molding (6) to the fender.
3. Install the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.

## Front Fender Body Side Molding Replacement Pontiac

### Removal Procedure

1. Remove the screws (3) at the wheel opening.
2. Remove the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.
3. Remove the fender insulator. Refer to Front Fender Insulator Replacement in Body Front End.
4. Remove the screw that retains the molding to the rocker panel (SSE only).
5. Gently pull the molding in order to disengage the clips.

### Installation Procedure

1. Press the molding in order to engage the clips.
2. Install the nuts to the backside of the fender.
3. Install the fender insulator. Refer to Front Fender Insulator Replacement in Body Front End.
4. Install the front wheelhouse panel. Refer to Wheelhouse Panel Replacement in Body Front End.
5. Install the screws (3) at the wheel opening.