For 1990-2009 cars

#### Tools Required

• | J 37096 Flywheel Holding Tool

• | J 38197-A Crankshaft Balancer Puller

1. Use J 37096 to hold the flywheel.
2. Remove the crankshaft balancer bolt.
3. Use the J 38197-A to remove the crankshaft balancer.

Important: Do not separate the crankshaft pulley from the crankshaft balancer. Service the crankshaft pulley and the crankshaft balancer as an assembly.

3.1. | Invert J 38197-2 so the leg of the tool is facing away from the crankshaft balancer.

3.2. | Install the silver screws J 38197-4 to the crankshaft balancer.

3.3. | Turn J 38197-1 to remove the crankshaft balancer from the crankshaft.

3.4. | Remove J 38197-1, J 38197-2, and J 38197-4 from the crankshaft balancer.