For 1990-2009 cars

## Roof Console Replacement Pontiac

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement .
2. Disconnect the roof console bezel (2) securing the overhead console cover (6) to the headliner.
3. Remove the fasteners retaining the overhead console (3) to the roof.
4. Remove the overhead console (3).

### Installation Procedure

1. Install the overhead console (3).
2. Install the retainers in order to secure the overhead console to the roof.
3. Install the overhead console cover (6) to the headliner (1).
4. Install the retainer (2) to secure the overhead console cover (6) to the headliner.
5. Install the headliner. Refer to Headlining Trim Panel Replacement .