For 1990-2009 cars

### Removal Procedure

1. Open the vanity cover (1).
2. Use a thin-bladed screwdriver in order to disengage the front snap legs (4) at the lower edge of the sunshade (5).
3. Pull the vanity out and down in order to remove the vanity.

Important: Note the wire routing for installation.

4. Disconnect the wire connectors from the vanity, if equipped.

### Installation Procedure

1. Partially install the vanity mirror assembly.
2. Connect the wire connectors, if equipped.
3. Insert the top end of the vanity into the sunshade.
4. Engage the snap legs (4).