For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 39384-3 Torque Rod Retaining Pin

• | J 39384-10 Torque Rod Adjustment Bar

1. Remove the trim panel between the rear seat and the rear window.
2. Remove the retainer clip from the torque rod (2) at the hinge (1).
3. From inside the vehicle, loosen, but do NOT remove, the 2 hinge retaining bolts.
4. Support the rear compartment lid.
5. Complete the following steps in order to relieve the tension on the torque rod (2):

5.1. | Insert the J 39384-3 in the hinge (1).

5.2. | Insert the J 39384-10 over the end of the torque rod (2).

6. Remove the torque rod (2) from the adjusting notches.

### Installation Procedure

#### Tools Required

• | J 39384-3 Torque Rod Retaining Pin

• | J 39384-10 Torque Rod Adjustment Bar

1. Install the torque rod (2) between the hinge (1) and the shelf.

Important: Properly seat the torque rod between the rear shelf and the hinge assembly.

2. Slide the torque rod (2) into the hinge (1). Secure the rod with the retainer.
3. Open and close the rear compartment lid in order to confirm that the torque rod (2) is seated properly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the hinge retaining bolts.

Tighten
Tighten the bolts to 18 N·m (13 lb ft).

5. Insert the torque rod into the adjustment notch:

5.1. | Insert the J 39384-3 in the hinge.

5.2. | Insert the J 39384-10 over the end of the torque rod.

6. Adjust the rear compartment lid to the desired tension. Refer to Rear Compartment Lid Adjustment .
7. Install the trim panel between the rear seat and the rear window.