For 1990-2009 cars

### Removal Procedure

1. Remove the wheel and the tire. Refer to Wheel Removal in Tires and Wheels.
2. Remove the brake drum. Refer to Brake Drum Replacement .
3. Remove the wheel stud using the J 6627-A .

### Installation Procedure

1. Install the new stud from the back side of the hub.
2. Install the four flat washers (1) on the stud.
3. Install the wheel nut with the flat side toward washers.
4. Tighten the nut (2) until the stud head is properly seated in the hub flange.
5. Install the brake drum. Brake Drum Replacement .

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the wheel and the tire.

Tighten
Tighten the wheel nuts to 140 N·m (100 lb ft).