For 1990-2009 cars

## Exhaust Manifold Installation Right Side

1. Install the right exhaust manifold gasket.
2. Install the right exhaust manifold.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the right exhaust manifold studs.

Tighten
Tighten the right exhaust manifold studs to 30 N·m (22 lb ft).

4. Install the fuel injector sight shield bracket.
5. Install the fuel injector sight shield bracket nuts.

Tighten
Tighten the fuel injector sight shield bracket nuts to 30 N·m (22 lb ft).

6. Install the right engine lift hook.
7. Install the right engine lift hook nut and bolt.

Tighten
Tighten the right engine lift hook nut and bolt to 30 N·m (22 lb ft).

8. Install the heated oxygen sensor lead.

Important: Inspect the EGR pipe for leaks during installation. If leaks are present, replace the EGR adapter assembly.

9. Install the EGR mounting bracket.
10. Install the EGR mounting bracket bolts.

Tighten
Tighten the EGR mounting bracket bolts to 50 N·m (37 lb ft).

11. Install the EGR inlet pipe to the exhaust manifold.
12. Install the EGR inlet pipe bolt.

Tighten
Tighten the EGR inlet pipe bolt to 29 N·m (21 lb ft).

## Exhaust Manifold Installation Left Side

1. Install the exhaust manifold gasket.
2. Install the exhaust manifold.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the exhaust manifold studs and bolt.

Tighten
Tighten the exhaust manifold studs and the exhaust manifold bolt to 30 N·m (22 lb ft).

4. Install the left engine lift hook.
5. Install the left engine lift hook nut and bolt.

Tighten
Tighten the left engine lift hook nut and bolt to 30 N·m (22 lb ft).